Skip to main content
`Ctrl`+`K`
scipy.signal.ShortTimeFFT.

# scipy.signal.ShortTimeFFT.lower_border_end

property ShortTimeFFT.lower_border_end

  First signal index and first slice index unaffected by pre-padding.

  Describes the point where the window does not stick out to the left of the signal domain. A detailed example is provided in the Sliding Windows section of the SciPy User Guide.

  See also

  `k_min`

    The smallest possible signal index.

  `k_max`

    First sample index after signal end not touched by a time slice.

  `lower_border_end`

    Where pre-padding effects end.

  `p_min`

    The smallest possible slice index.

  `p_max`

    Index of first non-overlapping upper time slice.

  `p_num`

    Number of time slices, i.e., `p_max` - `p_min`.

  `p_range`

    Determine and validate slice index range.

  `upper_border_begin`

    Where post-padding effects start.

  `ShortTimeFFT`

    Class this property belongs to.